### 2.3.4 Summary to: Conductors - Special Applications

| Thermionic emission provides electron beams. The electron beam current (density) is given by the Richardson equation: |  |
j = A · T 2 · exp – | EA kT
--- | ---
|  | Atheo = 120 A · cm–2 · K–2 for free electron gas model Aexp » (20 - 160) A · cm–2 · K–2 |
|  | EA = work function » (2 - >6) eV |
|  | Materials of choice: W, LaB6 single crystal |
| High field effects (tunneling, barrier lowering) allow large currents at low T from small (nm) size emitter |  |
Needs UHV!
| There are several thermoelectric effects for metal junctions; always encountered in non-equilibrium. |  |
|  | Seebeck effect: Thermovoltage develops if a metal A-metal B junction is at a temperature different form the "rest", i.e. if there is a temperature gradeient |  |
Essential for measuring (high) temperatures with a "thermoelement" Future use for efficient conversion of heat to electricity ???
Questionaire
All Multiple Choice questions to 2.3

© H. Föll (Electronic Materials - Script)